[EN]
1. To work with JTDX/WSJTX (or some other data mode softwares), add CI-V commands 0x25,0x26,
   See <<XIEGU RADIO CI-V REFERENCE>> and <<XIEGU RADIO JTDX WSJTX SETTINGs>>
2. Add CI-V command 0x1d 0x19, read the XIEGU RADIO ID,
   See <<XIEGU RADIO CI-V REFERENCE>>
3. Bug fix: Can't totally mute when RX volum set to 0
4. Bug fix: ACC TRX Pin is output only (now it's bidirectional)
5. Bug fix: Won't lock the long press key
6. Set RX audio bandwidth to 10~3300Hz in data mode