;This is a copy of the default version of PTC-2E.CMD.
;
;This is a sample TNC initialisation file for use with
;the Kenwood SCS PTC-2E.

[SETUP]
;DON'T alter anything in this section unless you are
;sure you know what you are doing!
COMMAND_PROMPT=
COMMAND_CHARACTER_CODE=
CONV_COMMAND=
MYCALL_COMMAND="^[mycall "
UNPROTO_COMMAND="^[C "
ESCAPE_CHARACTER_CODE=27
NO_BEACON_COMMAND=

[INIT_COMMANDS]
;two times quit to be sure that the Ptc-2e is in command mode in pactor
^[q
^[q
;terminal parameter for dumb terminal
^[term 0
;set the packet channel to the monitor channel
^[pac S 0
;set txdelay to 400msec (depends on your transmitter, can be shorter
;with a dedicated transmitter)
^[pac Txd 400
;set monitor to all
^[pac Mon 6
;set users to 0, so all incoming connects are routed to the Ptc-2e mailbox
^[pac user 0
;set radio baudrate (1k2, 9k6 is possible)
^[pac baud 1200
; set light diodes to bright - visual control if the command is executed
^[bri 6
; set the ptc2e into Packet mode
^[pac
; send convers command (only once necessary)
^[conv

[EXIT_COMMANDS]
; quit twice to be sure...
^[q
^[q
; set monitor to none
^[pac Mon 0
; set baudrate back to normal (depends on your normal packet operation)
^[pac baud 9600
; dim Led brightness to save energy
^[bri 1
; set back to Packet mode, depends on your favorite standby mode
^[pac
