;This is a copy of the default version of GES GC12AX.CMD.
;
;This is a sample TNC initialisation file for use with
;GES GC12AX's and clones.

[SETUP]
;DON'T alter anything in this section unless you
;are sure you know what you are doing!
COMMAND_PROMPT=cmd:
COMMAND_CHARACTER_CODE=3
ESCAPE_CHARACTER_CODE=
CONV_COMMAND=CONV
MYCALL_COMMAND="MYCALL "
UNPROTO_COMMAND="UNPROTO "
NO_BEACON_COMMAND=BEACON EVERY 0

[INIT_COMMANDS]
ECHO OFF
T 25
P 64
N 30
Y 10
@K

[EXIT_COMMANDS]
QRES
