;This is a copy of the default version of PK-232.CMD.
;
;This is a sample TNC initialisation file for use with
;the AEA/Timewave PK-232 and similar TNCs. It is the same
;as PK-232.CMD, but it has extra commands to recover the
;TNC from an unknown state. It is able to -
; 1. Auto-baud the TNC.
; 2. Take the TNC out of host mode or KISS mode.
;
;However, it take slightly longer to run than PK-232.CMD.

[SETUP]
;DON'T alter anything in this section unless you
;are sure you know what you are doing!
COMMAND_PROMPT=cmd:
COMMAND_CHARACTER_CODE=3
ESCAPE_CHARACTER_CODE=
CONV_COMMAND=CONV
MYCALL_COMMAND="MYCALL "
UNPROTO_COMMAND="UNPROTO "
NO_BEACON_COMMAND=BEACON EVERY 0

[INIT_COMMANDS]
*~!cmd:!2
^C^C^C~!cmd:!2
EXPERT ON
ECHO OFF
AWLEN 8
8BIT ON
PACKET
ACRDISP 0
BBSMSGS OFF
MFILTER $0
HEADER ON
BEACON EVERY 0
NEWMODE ON
NOMODE OFF
CONOK OFF
SENDPAC $0D
PACLEN 250
MON 6
PASSALL OFF

[EXIT_COMMANDS]
MON 0
